**WEEKEND**Art**7**.nr**0**117**1**2-**0**01

## Separett 公司的Weekend无水马桶，大小便分开，适合于乡村别墅、客房、公寓、车船等场合。内置风扇让屋内保持通风和没有臭味。

Weekend 配备一个12V风扇，电池线，还有可用来配合电池、太阳能板和电网联接的蓄电池。.

使用人数:

如果及时清理粪桶，人数不受限制。

# EASY TO USE很容易使用


## 内置粪桶

大便 落入内置粪桶内，尿液经前部尿盆流到马桶后而的尿液收集壶或者Separett Ejektortank尿液喷洒专用桶。

## EASY TO CLEAN容易清洁

很容易更换粪桶

当粪桶积满后，把桶提出来。加上 Roslagskompos后，大便 可以直接堆肥。如果要直接把大便埋在土里，需要把粪桶密封搁置12个月以上。 换气扇

12V风扇，配一个变压器，可让马桶能同12V电源和230V电网连接。

用一块湿布和中性清洁剂就可把马桶清洁干净。经常 用水冲洗一下尿盆也可以让尿管防止结晶堵塞。

**WEEKEND 7010 标配**

* 通风管 40 cm Ø75 mm –防蝇网
* 防雨垫 – 90°弯管 – 风帽
* 2 个大便桶 – 2个盖子
* 10 个可降解塑料袋

选配

* 1013-03 尿液喷洒桶\* – 1118-01生物除臭剂\*\*– 1198-01 清洁套装\*\*\* – 安装材料\*\*\*\*
	+ 2 m 尿管 Ø32 mm
	+ 密封硅胶
	+ 安装螺丝

\*

With an Ejektortank connected to the toilet its easy to make your own nutrient for your garden.

\*\*

Bio drain cleaner to help keep the urine drain free from urine salts that can clog the urine hose.

\*\*\*

Cleaning kit with all the things you need to keep your Weekend clean.

# INSTALLATION安装

排气管直安装在马桶后面，固定在墙壁上。对于 Weekend 7010来说，要用一个 12 V 风扇、一个90度弯管和4米排气管。尿液处理方式同 Villa 9000一样，最好同Separett专用尿液Ejektortank.

安装材料\*\*\*\*

Alternative 1第一种安装方法:

* + 1020-03 通风管

如果通风管太小，需要.:

 **r**

灰水

**过滤 尿箱**

* + 1024-01连接套

如果通风管太大，需要.:

* + 1025-01 连接套

连接灰水管，需要:

* + 1032-02 尿液接灰水套件

1020-03

1024-01 1025-01 1032-02

# TECHNICAL DATA

 497 mm

**WEEKEND 7010**

**无水马桶**

**大小便分离**

 450 mm

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **材质** | **粪桶** | **电压/ 功率** | **能耗** | **电线** | **噪音/重量**  | **包装尺寸/重量** |
| 可回收的耐冲击的聚氯乙烯 | 30L 聚氯乙烯,满桶： 10-12 kg | 12 V/2.5 W/210 mA | 0.396/0.276kWh/24 hrs | 电池线 1.9 m/ 变压器12/230V | <30 dB(A)150 kg | L:53 W:40 H:527 kg |

**Connections:**

532 mm

排气管: Ø75 mm

尿管: Ø32 mm

保质期3年.

所有电器部件都有 ETL 和/或 CE标志

其它信息见, [www.separett.com](http://www.separett.com/)

514 mm

155 mm

Separett AB 2018, 11980-01